# Munsell Color Conversion

Soil color is most often described using the Munsell color system. The `aqp` package provides several functions for converting to and from Munsell color notation, into other representations suitable for on-screen display (sRGB) or numerical analysis (CIELAB).

## Color Conversion Functions

Conversion of Munsell notation to “something” that can be displayed on-screen (sRGB color representation) is probably the most common color transformation applied to soil morphology data. The `munsell2rgb()` function is convenient for this operation when Munsell notation has been split into vectors of hue, value, and chroma. These could be columns in a `data.frame` or separate vectors. The `parseMunsell()` function is convenient when a full Munsell notation is given as a character vector. Note that `parseMunsell()` is a wrapper to `munsell2rgb()`. For example, converting `10YR 4/6` with either function can return:

- hex-notation of a color: `#805921FF`, or
- sRGB color coordinates: `0.5002233 0.3489249 0.1287694`, or
- CIELAB color coordinates: `40.95021 10.31088 37.49513`.

Selection of the closest `n` Munsell color “chips”, given sRGB or CIELAB colorspace coordinates is performed with the `col2Munsell()` function. Input to this function can be colorspace coordinates, named colors (e.g. `red`), or hex-notation of a color. For example, the selection of the closest Munsell chip for CIELAB coordinates `(51.4337, 9.917916, 38.6889)` results in `10YR 5/6` with a reported sigma (error) of `1.5e-6`. This error is estimated as the CIE2000 distance between the source CIELAB coordinates and the CIELAB coordinates of the closest Munsell chip.

A representative Munsell color can be estimated from reflectance spectra in the range of 380nm to 730nm with the `spec2Munsell()` function.

## Special Cases

Neutral colors are commonly specified two ways in the Munsell system: `N 3/` or `N 3/0`, either format will work with `munsell2rgb()` and `parseMunsell()`.

Non-standard Munsell notation (e.g. `3.6YR 4.4 / 5.6`), possibly collected with a sensor vs. color book, can be approximated with `getClosestMunsellChip()`. A more accurate conversion can be performed with the `munsellinterpol` package..

## Examples

    # Munsell -> hex color
    parseMunsell('5PB 4/6')

    #> [1] "#476189FF"

    # Munsell -> sRGB
    parseMunsell('5PB 4/6',  return_triplets = TRUE)

    #>           r         g         b
    #> 1 0.2774433 0.3816871 0.5373067

    # Munsell -> CIELAB
    parseMunsell('5PB 4/6',  returnLAB = TRUE)

    #>          L        A         B
    #> 1 40.78393 1.583845 -25.09816

    # hex color -> Munsell
    col2Munsell('#476189FF')

    #>   hue value chroma     sigma
    #> 1 5PB     4      6 0.2196242

    # neutral color
    parseMunsell('N 5/')

    #> [1] "#767676FF"

    # non-standard notation
    getClosestMunsellChip('3.3YR 4.4/6.1', convertColors = FALSE)

    #> [1] "2.5YR 4/6"